{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Calculated Metric - Setup Rules","Metric Setup Template"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Calculated Metric - Setup Rules","index":0,"n_rows":7,"n_cols":13,"rows_kept":7,"cut":false,"hidden":false,"merged":[[3,0,3,12],[4,0,4,12],[5,0,5,12],[6,0,6,12]]}
["Facility","Metric Category","Metric Name","Expected Input Type","UOM","Chemical Group (if applicable)","Reporting Granularity","Chart Type","What to Chart","Chart Values Should Be","Calculated Metric","Calculation","Notes"]
["Required. Enter each applicable facility name exactly as configured in EHS-Dashboard. Use a separate row when each facility requires its own calculated result. If one shared or aggregated metric intentionally applies to multiple facilities, separate the exact names with a comma and one space. Do not use abbreviations, semicolons, or line breaks.","Required. Use an existing Metric Category name exactly as it appears in EHS-Dashboard. If the category does not exist, create it before importing the metric.","Required. Enter a clear, specific name for the Calculated Environmental Metric. The name should distinguish the calculated result from the Source Environmental Metric or Process Line used in the calculation.","Required. Enter Quantity.","Required. Enter the EHS-Dashboard unit of measure for the final calculated result using its exact spelling and capitalization.","Enter the applicable Chemical Group name exactly. Options: VOC, HAP, HOC, HYC, Acid, Ammonia, Greenhouse Gas, PM, CO, CO2, CO2e, SO2, NOx, and RTAP. If multiple groups apply, separate them with a comma and one space. Leave blank when no Chemical Group applies.","Required. Select one: Quarterly, Monthly, Weekly, Daily, or Annually. Do not add leading or trailing spaces.","Required. Select None, Line, Simple Bar, or Stacked Bar. Select None when the metric should not be charted.","Required only when Chart Type is anything other than None. Select the value to chart, such as Usage or Cost. Leave blank when Chart Type is None.","Required only when Chart Type is anything other than None. Select how values should be handled, such as Sums or Averages. Leave blank when Chart Type is None.","Required. Enter TRUE because this import sheet configures Calculated Environmental Metrics.","Required. Use Source IDs instead of Source names. Enclose a Source Environmental Metric or previously created Calculated Environmental Metric ID in curly braces, for example {16420}x12.34. For a Process Line, use backticks around Process Line ID:Usage Category:% Concentration, for example `975:ug:high`x12.34/2000. Usage Category codes: ae=Air Emission, sg=Storage, ug=Usage, saw=Waste, ww=Wastewater. Concentration codes: low=Low, mid=Midpoint, high=High.","Optional. Enter concise information that will help identify or review the metric, such as the calculation purpose, applicable permit or methodology, factor name or publication year, or location of supporting documentation."]
[]
["Additional configuration rules"]
["Use one Calculated Environmental Metric per row. Source Environmental Metric IDs can be found under Admin > Sources by adding the ID column to the Sources table. Process Line IDs can be found under Admin > Manage Process Lines by opening the Process Line for editing and using the last number in the page URL."]
["The curly braces around metric IDs and the backticks around Process Line references are required. Use the Source ID, not the Source name, and confirm the Process Line Usage Category and concentration codes before importing."]
["Keep the import data area clean: do not include blank rows, instructions, totals, section headings, or formulas among the rows that will be imported."]

{"sheet":"Metric Setup Template","index":1,"n_rows":517,"n_cols":13,"rows_kept":517,"cut":false,"hidden":false,"merged":[]}
["Facility","Metric Category","Metric Name","Expected Input Type","UOM","Chemical Group (if applicable)","Reporting Granularity","Chart Type","What to Chart","Chart Values Should Be","Calculated Metric","Calculation","Notes"]
["Building 1","Combustion Emissions","EU 19 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`990:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`990:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`990:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`990:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`990:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`990:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`990:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`990:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`990:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 19 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`990:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`991:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`991:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`991:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`991:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`991:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`991:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`991:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`991:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`991:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 20 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`991:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`992:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`992:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`992:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`992:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`992:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`992:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`992:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`992:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`992:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 22 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`992:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`993:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`993:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`993:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`993:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`993:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`993:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`993:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`993:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`993:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 23 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`993:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`994:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`994:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`994:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`994:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`994:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`994:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`994:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`994:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`994:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 24 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`994:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`995:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`995:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`995:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`995:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`995:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`995:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`995:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`995:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`995:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 26 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`995:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`996:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`996:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`996:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`996:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`996:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`996:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`996:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`996:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`996:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 46 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`996:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`997:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`997:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`997:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`997:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`997:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`997:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`997:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`997:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`997:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 47 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`997:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`995:ug:high`x2.03742/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`998:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`998:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`998:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`998:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`998:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`998:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`998:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`998:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 48 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`998:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`999:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`999:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`999:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`999:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`999:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`999:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`999:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`999:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`999:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 49 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`999:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1000:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1000:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1000:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1000:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1000:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1000:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1000:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1000:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1000:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 50 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1000:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1001:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1001:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1001:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1001:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1001:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1001:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1001:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1001:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1001:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 51 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1001:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1002:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1002:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1002:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1002:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1002:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1002:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1002:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1002:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1002:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 52 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1002:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1003:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1003:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1003:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1003:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1003:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1003:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1003:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1003:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1003:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 53 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1003:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1004:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1004:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1004:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1004:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1004:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1004:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1004:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1004:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1004:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 54 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1004:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1005:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1005:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1005:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1005:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1005:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1005:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1005:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1005:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1005:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 67 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1005:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1006:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1006:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1006:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1006:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1006:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1006:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1006:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1006:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1006:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 68 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1006:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1007:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1007:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1007:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1007:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1007:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1007:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1007:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1007:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1007:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 69 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1007:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1008:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1008:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1008:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1008:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1008:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1008:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1008:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1008:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1008:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 70 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1008:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1009:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1009:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1009:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1009:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1009:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1009:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1009:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1009:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1009:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 6 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1009:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1010:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1010:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1010:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1010:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1010:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1010:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1010:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1010:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1010:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 7 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1010:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1011:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1011:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1011:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1011:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1011:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1011:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1011:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1011:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1011:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 8 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1011:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1012:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1012:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1012:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1012:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1012:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1012:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1012:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1012:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1012:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 9 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1012:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1013:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1013:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1013:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1013:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1013:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1013:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1013:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1013:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1013:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 10 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1013:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1014:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1014:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1014:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1014:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1014:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1014:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1014:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1014:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1014:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 11 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1014:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1017:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1017:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1017:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1017:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1017:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1017:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1017:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1017:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1017:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 36 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1017:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1019:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1019:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1019:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1019:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1019:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1019:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1019:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1019:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1019:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 39 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1019:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1020:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1020:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1020:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1020:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1020:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1020:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1020:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1020:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1020:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 40 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1020:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1021:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1021:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1021:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1021:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1021:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1021:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1021:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1021:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1021:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 41 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1021:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1022:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1022:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1022:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1022:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1022:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1022:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1022:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1022:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1022:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 42 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1022:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1023:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1023:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1023:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1023:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1023:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1023:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1023:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1023:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1023:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 43 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1023:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1024:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1024:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1024:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1024:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1024:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1024:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1024:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1024:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1024:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 44 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1024:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1025:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1025:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1025:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1025:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1025:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1025:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1025:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1025:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1025:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 45 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1025:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1026:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1026:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1026:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1026:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1026:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1026:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1026:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1026:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1026:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 62 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1026:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1027:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1027:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1027:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1027:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1027:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1027:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1027:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1027:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1027:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 63 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1027:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1028:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1028:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1028:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1028:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1028:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1028:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1028:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1028:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1028:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 64 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1028:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1029:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1029:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1029:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1029:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1029:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1029:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1029:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1029:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1029:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 65 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1029:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1030:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM10 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1030:ug:high`x1.9/1037x0.1/2000","1.9 lb/MMCF = PM2.5 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1030:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1030:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1030:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1030:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1030:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1030:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1030:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 66 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1030:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1015:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM10 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1015:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM2.5 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1015:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1015:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1015:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1015:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1015:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1015:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1015:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 14 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1015:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1016:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM10 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1016:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM2.5 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1016:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1016:ug:high`x68/1037x0.1/2000","68 lb/MMCF = NOx EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1016:ug:high`x76/1037x0.1/2000","76 lb/MMCF = CO EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1016:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1016:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1016:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1016:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 15 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1016:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1041:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM10 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1041:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM2.5 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1041:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1041:ug:high`x100/1037x0.1/2000","100 lb/MMCF = NOx EF (Source Registration RY 2014 - AP1 Forms (Nat Gas <10 MMBtu/hr)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1041:ug:high`x84/1037x0.1/2000","84 lb/MMCF = CO EF (Source Registration RY 2014 - AP1 Forms (Nat Gas <10 MMBtu/hr)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1041:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1041:ug:high`x0.49/1037x0.1/2000","0.49 lb/MMCF = NH3 EF (Source Registration RY 2014 - AP1 Forms (Nat Gas <10 MMBtu/hr)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1041:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1041:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 7-ALE N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1041:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1037:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM10 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1037:ug:high`x7.6/1037x0.1/2000","7.6 lb/MMCF = PM2.5 EF (ERP), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1037:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (AP-42 standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1037:ug:high`x100/1037x0.1/2000","100 lb/MMCF = NOx EF (Source Registration RY 2014 - AP1 Forms (Nat Gas <10 MMBtu/hr)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1037:ug:high`x84/1037x0.1/2000","84 lb/MMCF = CO EF (Source Registration RY 2014 - AP1 Forms (Nat Gas <10 MMBtu/hr)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1037:ug:high`x5.5/1037x0.1/2000","5.5 lb/MMCF = VOC EF (Facility RES permit), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1037:ug:high`x0.49/1037x0.1/2000","0.49 lb/MMCF = NH3 EF (Source Registration RY 2014 - AP1 Forms (Nat Gas <10 MMBtu/hr)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1037:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1037:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 2 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1037:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1038:ug:high`x3/1037x0.1/2000","3 lb/MMCF = PM10 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1038:ug:high`x3/1037x0.1/2000","3 lb/MMCF = PM2.5 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1038:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1038:ug:high`x100/1037x0.1/2000","100 lb/MMCF = NOx EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1038:ug:high`x20/1037x0.1/2000","20 lb/MMCF = CO EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1038:ug:high`x5.299/1037x0.1/2000","5.299 lb/MMCF = VOC EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1038:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"`1038:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1038:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 3 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1038:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1039:ug:high`x3/1037x0.1/2000","3 lb/MMCF = PM10 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1039:ug:high`x3/1037x0.1/2000","3 lb/MMCF = PM2.5 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1039:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1039:ug:high`x100/1037x0.1/2000","100 lb/MMCF = NOx EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1039:ug:high`x20/1037x0.1/2000","20 lb/MMCF = CO EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1039:ug:high`x5.299/1037x0.1/2000","5.299 lb/MMCF = VOC EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1039:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"`1039:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1039:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 4 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1039:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1040:ug:high`x3/1037x0.1/2000","3 lb/MMCF = PM10 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1040:ug:high`x3/1037x0.1/2000","3 lb/MMCF = PM2.5 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"`1040:ug:high`x0.6/1037x0.1/2000","0.6 lb/MMCF = SO2 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"`1040:ug:high`x100/1037x0.1/2000","100 lb/MMCF = NOx EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"`1040:ug:high`x20/1037x0.1/2000","20 lb/MMCF = CO EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"`1040:ug:high`x5.299/1037x0.1/2000","5.299 lb/MMCF = VOC EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"`1040:ug:high`x3.2/1037x0.1/2000","3.2 lb/MMCF = NH3 EF (Source Registration RY 2014 - AP1 Forms (Space Heater)), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"`1040:ug:high`x120026.676/1037x0.1/2000","120026.676 lb/MMCF = CO2 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1040:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = CH4 EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 5 N2O Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"`1040:ug:high`x2.03742/1037x0.1/2000","2.03742 lb/MMCF = N2O EF (CRIS standard emission factor), 1037 Btu/CF = Natural Gas Heat Content, 0.1 MMBtu = 1 Therm, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"`1037:ug:high`x2.03742/1037x0.1/2000","0.31 lb/MMBtu = PM10 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16643}x0.31x0.14/2000","0.31 lb/MMBtu = PM2.5 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"{16643}x0.29x0.14/2000","0.29 lb/MMBtu = SO2 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16643}x4.41x0.14/2000","4.41 lb/MMBtu = NOx EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"{16643}x0.95x0.14/2000","0.95 lb/MMBtu = CO EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16643}x0.35x0.14/2000","0.35 lb/MMBtu = VOC EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16643}x0.020714286x0.14/2000","0.020714286 lb/MMBtu = NH3 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16643}x160.4428571x0.14/2000","160.4428571 lb/MMBtu = CO2 EF (CRIS standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 27 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16643}x0.008611429x0.14/2000","0.008611429 lb/MMBtu = CH4 EF (CRIS standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16644}x0.31x0.14/2000","0.31 lb/MMBtu = PM10 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16644}x0.31x0.14/2000","0.31 lb/MMBtu = PM2.5 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"{16644}x0.29x0.14/2000","0.29 lb/MMBtu = SO2 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16644}x4.41x0.14/2000","4.41 lb/MMBtu = NOx EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"{16644}x0.95x0.14/2000","0.95 lb/MMBtu = CO EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16644}x0.35x0.14/2000","0.35 lb/MMBtu = VOC EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16644}x0.020714286x0.14/2000","0.020714286 lb/MMBtu = NH3 EF (AP-42 standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16644}x160.4428571x0.14/2000","160.4428571 lb/MMBtu = CO2 EF (CRIS standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 28 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16644}x0.008611429x0.14/2000","0.008611429 lb/MMBtu = CH4 EF (CRIS standard emission factor), 0.14 MMBtu = 1 gal Diesel, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16645}x1600x0.0904/453.592/2000","1600 kW = EU55 Power Rating, 0.0904 g/kW-hr = PM10 EF (ERP, with N2CR Catalyst), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16645}x1600x0.0904/453.592/2000","1600 kW = EU55 Power Rating, 0.0904 g/kW-hr = PM2.5 EF (ERP, with N2CR Catalyst), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16645}x1600x0.5/453.592/2000","1600 kW = EU55 Power Rating, 0.5 g/kW-hr = NOx EF (ERP, with N2CR Catalyst), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"{16645}x1600x0.048/453.592/2000","1600 kW = EU55 Power Rating, 0.048 g/kW-hr = CO EF (ERP, with N2CR Catalyst), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16645}x1600x0.104/453.592/2000","1600 kW = EU55 Power Rating, 0.104 g/kW-hr = VOC EF (ERP, with N2CR Catalyst), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16645}x1600x0.1058217/453.592/2000","1600 kW = EU55 Power Rating, 0.1058217 g/kW-hr = NH3 EF (AP-42 standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"{16645}x1600x819.6439955/453.592/2000","1600 kW = EU55 Power Rating, 819.6439955 g/kW-hr = CO2 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 55 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16645}x1600x0.0439926/453.592/2000","1600 kW = EU55 Power Rating, 0.0439926 g/kW-hr = CH4 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16646}x800x0.2/453.592/2000","800 kW = EU13 Power Rating, 0.2 g/kW-hr = PM10 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16646}x800x0.2/453.592/2000","800 kW = EU13 Power Rating, 0.2 g/kW-hr = PM2.5 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16646}x800x6.4/453.592/2000","800 kW = EU13 Power Rating, 6.4 g/kW-hr = NOx EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"{16646}x800x3.5/453.592/2000","800 kW = EU13 Power Rating, 3.5 g/kW-hr = CO EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16646}x800x6.4/453.592/2000","800 kW = EU13 Power Rating, 6.4 g/kW-hr = VOC EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16646}x800x0.09380775/453.592/2000","800 kW = EU13 Power Rating, 0.09380775 g/kW-hr = NH3 EF (AP-42 standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"{16646}x800x726.589545/453.592/2000","800 kW = EU13 Power Rating, 726.589545 g/kW-hr = CO2 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 2","Combustion Emissions","EU 13 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16646}x800x0.038998146/453.592/2000","800 kW = EU13 Power Rating, 0.038998146 g/kW-hr = CH4 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16647}x1500x0.065/453.592/2000","1500 kW = EU16 Power Rating, 0.065 g/kW-hr = PM10 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16647}x1500x0.065/453.592/2000","1500 kW = EU16 Power Rating, 0.065 g/kW-hr = PM2.5 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16647}x1500x7.012/453.592/2000","1500 kW = EU16 Power Rating, 7.012 g/kW-hr = NOx EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"{16647}x1500x0.664/453.592/2000","1500 kW = EU16 Power Rating, 0.664 g/kW-hr = CO EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16647}x1500x0.158/453.592/2000","1500 kW = EU16 Power Rating, 0.158 g/kW-hr = VOC EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16647}x1500x0.098306133/453.592/2000","1500 kW = EU16 Power Rating, 0.098306133 g/kW-hr = NH3 EF (AP-42 standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"{16647}x1500x761.4318507/453.592/2000","1500 kW = EU16 Power Rating, 761.4318507 g/kW-hr = CO2 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 16 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16647}x1500x0.040868233/453.592/2000","1500 kW = EU16 Power Rating, 0.040868233 g/kW-hr = CH4 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16648}x2250x0.065/453.592/2000","2250 kW = EU17 Power Rating, 0.065 g/kW-hr = PM10 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16648}x2250x0.065/453.592/2000","2250 kW = EU17 Power Rating, 0.065 g/kW-hr = PM2.5 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16648}x2250x7.174/453.592/2000","2250 kW = EU17 Power Rating, 7.174 g/kW-hr = NOx EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"{16648}x2250x0.943/453.592/2000","2250 kW = EU17 Power Rating, 0.943 g/kW-hr = CO EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16648}x2250x0.12/453.592/2000","2250 kW = EU17 Power Rating, 0.12 g/kW-hr = VOC EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16648}x2250x0.095789964/453.592/2000","2250 kW = EU17 Power Rating, 0.095789964 g/kW-hr = NH3 EF (AP-42 standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"{16648}x2250x741.9428212/453.592/2000","2250 kW = EU17 Power Rating, 741.9428212 g/kW-hr = CO2 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 17 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16648}x2250x0.0398222/453.592/2000","2250 kW = EU17 Power Rating, 0.0398222 g/kW-hr = CH4 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16649}x400x0.09/453.592/2000","400 kW = EU61 Power Rating, 0.09 g/kW-hr = PM10 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16649}x400x0.09/453.592/2000","400 kW = EU61 Power Rating, 0.09 g/kW-hr = PM2.5 EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16649}x400x5.37/453.592/2000","400 kW = EU61 Power Rating, 5.37 g/kW-hr = NOx EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 CO Emissions Tons","Quantity","ton","CO","Monthly ",null,null,null,true,"{16649}x400x1.6/453.592/2000","400 kW = EU61 Power Rating, 1.6 g/kW-hr = CO EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16649}x400x5.5/453.592/2000","400 kW = EU61 Power Rating, 5.5 g/kW-hr = VOC EF (ERP), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16649}x400x0.10434/453.592/2000","400 kW = EU61 Power Rating, 0.10434 g/kW-hr = NH3 EF (AP-42 standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 CO2 Emissions Tons","Quantity","ton","CO2","Monthly ",null,null,null,true,"{16649}x400x808.172/453.592/2000","400 kW = EU61 Power Rating, 808.172 g/kW-hr = CO2 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Building 1","Combustion Emissions","EU 61 CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16649}x400x0.04338/453.592/2000","400 kW = EU61 Power Rating, 0.04338 g/kW-hr = CH4 EF (CRIS standard emission factor), 453.592 g = 1 lb, 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE SO2 Emissions Tons","Quantity","ton","SO2","Monthly ",null,null,null,true,"{16655}x0.13938/2000","0.13938 lb/gal = SO2 EF (Source Registration RY 2014 - AP1 Forms), 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE VOC Emissions Tons","Quantity","ton","VOC","Monthly ",null,null,null,true,"{16655}x0.00005658/2000","0.00005658 lb/gal = VOC EF (Source Registration RY 2014 - AP1 Forms), 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE NH3 Emissions Tons","Quantity","ton","Ammonia","Monthly ",null,null,null,true,"{16655}x0.91356/2000","0.91356 lb/gal = NH3 EF (Source Registration RY 2014 - AP1 Forms), 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE CO2 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16655}x22.462/2000","22.462 lb/gal = CO2 EF (CRIS standard emission factor), 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE CH4 Emissions Tons","Quantity","ton","Greenhouse Gas","Monthly ",null,null,null,true,"{16655}x0.0012056/2000","0.0012056 lb/gal = CH4 EF (CRIS standard emission factor), 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE PM10 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16656}x0.25/2000","0.25 lb/hr = PM10 EF (Generator Emissions Spec Sheet for Potential Site Variation), 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE PM2.5 Emissions Tons","Quantity","ton","PM","Monthly ",null,null,null,true,"{16656}x0.25/2000","0.25 lb/hr = PM2.5 EF (Generator Emissions Spec Sheet for Potential Site Variation), 2000 lb/US ton"]
["Project 1","Combustion Emissions","EU 6-ALE NOx Emissions Tons","Quantity","ton","Nox","Monthly ",null,null,null,true,"{16656}x8.33/2000","8.33 lb/hr = NOx EF (Generator Emissions Spec Sheet for Potential Site Variation), 2000 lb/US ton"]